New Features in 2.0.343
SDI Generator with Auto Gen mode.
2K video support.
SDI 96kHz audio sample rates.
De-embedding of extended groups.
Test tone generator in the de-embedder path.
Separate SRC bypass control for embed and de-embed paths.

Firmware Note:
If you experience any interoperability or stability issues with the latest firmware, please try the previous version (v1.7.292) included in this folder, which may offer improved compatibility with certain systems. We recommend resetting the unit back to defaults after loading the firmware.

